|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Device name | Equipment type | Drive type | IP | Port | COM | Baud rate |
| Eye | Electric eye | Serial port |  |  | Com1 | 9600 |
| Case rejector | Reject device | Serial port |  |  | Com5 | 9600 |
| Case scanner | Scan device | Socket | 192.168.3.200 | 51236 |  |  |
| Scan qun | Scan device | Serial port |  |  | Com6 | 9600 |
| Bottle rejector | Reject device | Serial port |  |  | Com3 | 9600 |
| Bottle scanner | Scan device | Socket | 192.168.100.100 | 9004 |  |  |

KT5 ^

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Device name | Equipment type | Drive type | IP | Port | COM | Baud rate |
| Box printer | Scan device | Serial port |  |  | Com10 | 9600 |
| Bottle printer | Scan device | Serial port |  |  | Com11 | 9600 |
| Case rejector | Reject device | Serial port |  |  | Com4 |  |
| Case scanner | Scan device | Socket | 192.168.3.200 | 51236 |  |  |
| Scan qun | Scan device | Serial port |  |  | Com7 | 7200 |
| Bottle rejector | Reject device | Serial port |  |  | Com5 | 9600 |
| Bottle scanner | Scan device | Socket | 192.168.3.100 | 51236 |  |  |

KT7 ^

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Device name | Equipment type | Drive type | IP | Port | COM | Baud rate |
| Box Reject | Reject device | Serial port |  |  | Com2 | 9600 |
| Select Scan | Scan device | Serial port |  |  | Com6 | 9600 |
| Box Scan | Scan device | Socket | 192.168.3.200 | 51236 |  |  |
| Bottle Reject | Reject device | Serial port |  |  | Com1 | 9600 |
| Bottle Scan | Scan device | Socket | 192.168.3.100 | 51236 |  |  |

KT12 ^